Highligths:

1. We simulate gas-liquid mass transfer for bubble train flow
2. The bubble shapes are obtained numerically without analytical simplifications
3. The lattice Boltzmann method was used for mass transfer and flow simulations

4. One unit cell simulations are enough to obtain the correct mass transfer coefficient