Highlights:

* We simulate gas-liquid mass transfer for bubble train flow
* The bubble shapes are obtained numerically without analytical simplifications
* The lattice Boltzmann method was used for mass transfer and flow simulations
* One unit cell simulations are enough to obtain the correct mass transfer coefficient